<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.11-Bratislava">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>BOUNDCRS[SOURCECRS[PROJCRS["Mexico_ITRF2008_LCC",BASEGEOGCRS["Mexico_ITRF2008",DATUM["Mexico ITRF2008",ELLIPSOID["GRS_1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["Degree",0.0174532925199433]]],CONVERSION["unnamed",METHOD["Lambert Conic Conformal (2SP)",ID["EPSG",9802]],PARAMETER["Longitude of false origin",-102,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8822]],PARAMETER["Latitude of false origin",12,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8821]],PARAMETER["Easting at false origin",2500000,LENGTHUNIT["Meter",1],ID["EPSG",8826]],PARAMETER["Northing at false origin",0,LENGTHUNIT["Meter",1],ID["EPSG",8827]],PARAMETER["Latitude of 1st standard parallel",17.5,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8823]],PARAMETER["Latitude of 2nd standard parallel",29.5,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8824]],PARAMETER["Scale_Factor",1,SCALEUNIT["unity",1]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["Meter",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["Meter",1]],ID["EPSG",6372]]],TARGETCRS[GEOGCRS["WGS 84",DATUM["World Geodetic System 1984",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]]],ABRIDGEDTRANSFORMATION["Transformation from Mexico_ITRF2008 to WGS84",METHOD["Position Vector transformation (geog2D domain)",ID["EPSG",9606]],PARAMETER["X-axis translation",0,ID["EPSG",8605]],PARAMETER["Y-axis translation",0,ID["EPSG",8606]],PARAMETER["Z-axis translation",0,ID["EPSG",8607]],PARAMETER["X-axis rotation",0,ID["EPSG",8608]],PARAMETER["Y-axis rotation",0,ID["EPSG",8609]],PARAMETER["Z-axis rotation",0,ID["EPSG",8610]],PARAMETER["Scale difference",1,ID["EPSG",8611]]]]</wkt>
      <proj4>+proj=lcc +lat_0=12 +lon_0=-102 +lat_1=17.5 +lat_2=29.5 +x_0=2500000 +y_0=0 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs +type=crs</proj4>
      <srsid>0</srsid>
      <srid>0</srid>
      <authid></authid>
      <description>Mexico_ITRF2008_LCC</description>
      <projectionacronym></projectionacronym>
      <ellipsoidacronym>PARAMETER:6378137:6356752.31414035614579916</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
